The high pressure transducer has the following characteristics:

input voltage: 9-36Vdc

output voltage: 1-5Vdc

part# G2 M01 15 F2 5000#